ThingSpeak Communication Library Enables an Arduino or ESP8266 to write or read data to or from ThingSpeak™ |

- Main Page
- Data Structures

- Data Structures
- Data Fields

- All
- Functions

- b
- g
- r
- s
- w

### - b -

- begin() : ThingSpeakClass

### - g -

- getLastReadStatus() : ThingSpeakClass

### - r -

- readCreatedAt() : ThingSpeakClass
- readFloatField() : ThingSpeakClass
- readIntField() : ThingSpeakClass
- readLongField() : ThingSpeakClass
- readRaw() : ThingSpeakClass
- readStatus() : ThingSpeakClass
- readStringField() : ThingSpeakClass

### - s -

- setCreatedAt() : ThingSpeakClass
- setElevation() : ThingSpeakClass
- setField() : ThingSpeakClass
- setLatitude() : ThingSpeakClass
- setLongitude() : ThingSpeakClass
- setStatus() : ThingSpeakClass
- setTwitterTweet() : ThingSpeakClass

### - w -

- writeField() : ThingSpeakClass
- writeFields() : ThingSpeakClass
- writeRaw() : ThingSpeakClass